FINISHED BOARDS
Enter Q.C. Tag Identification Code

REJECTS BY TYPE	TOTAL
1.	Circuit boards clean, unmarked & unchipped
2.	Wires & components fully inserted
3.	Proper location & positioning of components
4.	Red, black, & green wires in proper location
5.	Alarm leads in proper location
6.	Alarm properly installed
7.	Alarm positioned properly
8.	Diode polarity properly positioned
9.	Circuit test: Alarm goes off with battery connected at proper +/- poles
10.	Quality Control Tag completed properly
11.	Quality Control Tag properly affixed
LEGEND = REJECT

TOTAL